Static Call Graph - [17\17.axf]

# Static Call Graph for image 17\17.axf

#<CALLGRAPH># ARM Linker, 5060183: Last Updated: Mon Jan 30 14:09:27 2017

### Maximum Stack Usage = 192 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ STRING_NUM_L ⇒ FONT_OUT ⇒ LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT

### Mutually Recursive functions

- CAN1_RX1_IRQHandler ⇒ CAN1_RX1_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- Error_Handler ⇒ Error_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from stm32f1xx_it.o(i.ADC1_2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel3_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from stm32f1xx_it.o(i.FLASH_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from stm32f1xx_it.o(i.RCC_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from stm32f1xx_it.o(i.SPI1_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI_DMAError from stm32f1xx_hal_spi.o(i.SPI_DMAError) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_DMAHalfTransmitCplt from stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_DMATransmitCplt from stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_TxISR from stm32f1xx_hal_spi.o(i.SPI_TxISR) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from stm32f1xx_it.o(i.TIM2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART1_IRQHandler from stm32f1xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> CAN1_RX1_IRQHandler
  [Called By]
  - >> CAN1_RX1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  ADC1_2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.ADC1_2_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC1_2_IRQHandler ⇒ HAL_ADC_IRQHandler
  [Calls]
  - >> HAL_ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  ADC_ConversionStop_Disable (Thumb, 76 bytes, Stack size 16 bytes, stm32f1xx_hal_adc.o(i.ADC_ConversionStop_Disable))
  [Stack]

  - Max Depth = 16
  - Call Chain = ADC_ConversionStop_Disable
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_ADC_Stop
  - >> HAL_ADC_Init

  ADC_Enable (Thumb, 104 bytes, Stack size 24 bytes, stm32f1xx_hal_adc.o(i.ADC_Enable))
  [Stack]

  - Max Depth = 24
  - Call Chain = ADC_Enable
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_ADC_Start

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel3_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel3_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  Error_Handler (Thumb, 2 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Calls]

  - >> Error_Handler
  [Called By]
  - >> Error_Handler
  - >> HAL_SPI_MspInit

  FLASH_IRQHandler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.FLASH_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLASH_IRQHandler ⇒ HAL_FLASH_IRQHandler
  [Calls]
  - >> HAL_FLASH_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  FLASH_PageErase (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase))
  [Called By]

  - >> HAL_FLASH_IRQHandler
  - >> FLASH_WriteSettings

  FLASH_ReadSettings (Thumb, 10 bytes, Stack size 0 bytes, main.o(i.FLASH_ReadSettings))
  [Called By]

  - >> main

  FLASH_WriteSettings (Thumb, 56 bytes, Stack size 16 bytes, main.o(i.FLASH_WriteSettings))
  [Stack]

  - Max Depth = 40
  - Call Chain = FLASH_WriteSettings ⇒ HAL_FLASH_Program_IT
  [Calls]
  - >> FLASH_PageErase
  - >> HAL_FLASH_Unlock
  - >> HAL_FLASH_Program_IT
  - >> HAL_FLASH_Lock
  [Called By]
  - >> main

  FONT_OUT (Thumb, 266 bytes, Stack size 48 bytes, spi_tft.o(i.FONT_OUT))
  [Stack]

  - Max Depth = 120
  - Call Chain = FONT_OUT ⇒ LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_SPI_Transmit_DMA
  - >> LCD_SetCursorPosition
  - >> LCD_SendCommand
  - >> LCD_fillRect
  [Called By]
  - >> STRING_OUT
  - >> STRING_NUM_L

  GPIO_init (Thumb, 132 bytes, Stack size 56 bytes, spi_tft.o(i.GPIO_init))
  [Stack]

  - Max Depth = 96
  - Call Chain = GPIO_init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> LCD_Init

  HAL_ADCEx_InjectedConvCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedConvCpltCallback))
  [Called By]

  - >> HAL_ADC_IRQHandler

  HAL_ADC_ConfigChannel (Thumb, 346 bytes, Stack size 24 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_ADC_ConfigChannel
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_ConvCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback))
  [Called By]

  - >> HAL_ADC_IRQHandler

  HAL_ADC_GetValue (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_GetValue))
  [Called By]

  - >> main

  HAL_ADC_IRQHandler (Thumb, 230 bytes, Stack size 8 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_ADC_IRQHandler
  [Calls]
  - >> HAL_ADCEx_InjectedConvCpltCallback
  - >> HAL_ADC_LevelOutOfWindowCallback
  - >> HAL_ADC_ConvCpltCallback
  [Called By]
  - >> ADC1_2_IRQHandler

  HAL_ADC_Init (Thumb, 300 bytes, Stack size 24 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> ADC_ConversionStop_Disable
  - >> HAL_ADC_MspInit
  [Called By]
  - >> MX_ADC1_Init

  HAL_ADC_LevelOutOfWindowCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_LevelOutOfWindowCallback))
  [Called By]

  - >> HAL_ADC_IRQHandler

  HAL_ADC_MspInit (Thumb, 66 bytes, Stack size 24 bytes, stm32f1xx_hal_msp.o(i.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_ADC_Init

  HAL_ADC_PollForConversion (Thumb, 290 bytes, Stack size 32 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_PollForConversion))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_ADC_PollForConversion ⇒ HAL_RCCEx_GetPeriphCLKFreq
  [Calls]
  - >> HAL_GetTick
  - >> HAL_RCCEx_GetPeriphCLKFreq
  [Called By]
  - >> main

  HAL_ADC_Start (Thumb, 184 bytes, Stack size 16 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_Start))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_ADC_Start ⇒ ADC_Enable
  [Calls]
  - >> ADC_Enable
  [Called By]
  - >> main

  HAL_ADC_Stop (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_adc.o(i.HAL_ADC_Stop))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_ADC_Stop ⇒ ADC_ConversionStop_Disable
  [Calls]
  - >> ADC_ConversionStop_Disable
  [Called By]
  - >> main

  HAL_DMA_IRQHandler (Thumb, 616 bytes, Stack size 40 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA1_Channel3_IRQHandler

  HAL_DMA_Init (Thumb, 80 bytes, Stack size 16 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Init
  [Called By]
  - >> HAL_SPI_MspInit

  HAL_DMA_Start_IT (Thumb, 88 bytes, Stack size 16 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> DMA_SetConfig
  [Called By]
  - >> HAL_SPI_Transmit_DMA

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCC_OscConfig
  - >> LCD_Init
  - >> main

  HAL_FLASH_EndOfOperationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback))
  [Called By]

  - >> HAL_FLASH_IRQHandler

  HAL_FLASH_IRQHandler (Thumb, 256 bytes, Stack size 24 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_FLASH_IRQHandler
  [Calls]
  - >> HAL_FLASH_OperationErrorCallback
  - >> HAL_FLASH_EndOfOperationCallback
  - >> FLASH_PageErase
  - >> FLASH_SetErrorCode
  - >> FLASH_Program_HalfWord
  [Called By]
  - >> FLASH_IRQHandler

  HAL_FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Lock))
  [Called By]

  - >> FLASH_WriteSettings

  HAL_FLASH_OperationErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback))
  [Called By]

  - >> HAL_FLASH_IRQHandler

  HAL_FLASH_Program_IT (Thumb, 92 bytes, Stack size 24 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Program_IT))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_FLASH_Program_IT
  [Calls]
  - >> FLASH_Program_HalfWord
  [Called By]
  - >> FLASH_WriteSettings

  HAL_FLASH_Unlock (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Unlock))
  [Called By]

  - >> FLASH_WriteSettings

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> GPIO_init
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit
  - >> HAL_SPI_MspInit
  - >> HAL_ADC_MspInit

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> main

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> LCD_SendData
  - >> LCD_SendCommand
  - >> GPIO_init
  - >> FONT_OUT
  - >> LCD_fillRect
  - >> LCD_Fill
  - >> main
  - >> MX_GPIO_Init
  - >> TIM2_IRQHandler

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> ADC_Enable
  - >> ADC_ConversionStop_Disable
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_ADC_PollForConversion
  - >> SPI_WaitOnFlagUntilTimeout

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 150 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> main
  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> HAL_SPI_MspInit
  - >> HAL_MspInit
  - >> HAL_ADC_MspInit

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> main
  - >> SystemClock_Config
  - >> HAL_UART_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> HAL_SPI_MspInit
  - >> HAL_MspInit
  - >> HAL_ADC_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init
  - >> HAL_MspInit

  HAL_RCCEx_GetPeriphCLKFreq (Thumb, 208 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCCEx_GetPeriphCLKFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_ADC_PollForConversion

  HAL_RCCEx_PeriphCLKConfig (Thumb, 288 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_CSSCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_CSSCallback))
  [Called By]

  - >> HAL_RCC_NMI_IRQHandler

  HAL_RCC_ClockConfig (Thumb, 374 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_EnableCSS (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_EnableCSS))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 34 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 34 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 102 bytes, Stack size 28 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_NMI_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RCC_NMI_IRQHandler
  [Calls]
  - >> HAL_RCC_CSSCallback
  [Called By]
  - >> NMI_Handler

  HAL_RCC_OscConfig (Thumb, 1406 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SPI_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_ErrorCallback))
  [Called By]

  - >> HAL_SPI_IRQHandler
  - >> SPI_TxCloseIRQHandler
  - >> SPI_DMATransmitCplt
  - >> SPI_DMAError

  HAL_SPI_IRQHandler (Thumb, 176 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SPI_IRQHandler
  [Calls]
  - >> HAL_SPI_ErrorCallback
  [Called By]
  - >> SPI1_IRQHandler

  HAL_SPI_Init (Thumb, 132 bytes, Stack size 8 bytes, stm32f1xx_hal_spi_ex.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> MX_SPI1_Init

  HAL_SPI_MspInit (Thumb, 134 bytes, Stack size 40 bytes, stm32f1xx_hal_msp.o(i.HAL_SPI_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> HAL_DMA_Init
  - >> Error_Handler
  [Called By]
  - >> HAL_SPI_Init

  HAL_SPI_Transmit_DMA (Thumb, 178 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_SPI_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> FONT_OUT
  - >> LCD_fillRect
  - >> LCD_Fill

  HAL_SPI_Transmit_IT (Thumb, 158 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SPI_Transmit_IT
  [Called By]
  - >> LCD_SendData
  - >> LCD_SendCommand

  HAL_SPI_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_TxCpltCallback))
  [Called By]

  - >> SPI_TxCloseIRQHandler
  - >> SPI_DMATransmitCplt

  HAL_SPI_TxHalfCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_TxHalfCpltCallback))
  [Called By]

  - >> SPI_DMAHalfTransmitCplt

  HAL_SPI_TxRxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback))
  [Called By]

  - >> SPI_TxCloseIRQHandler

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 80 bytes, Stack size 12 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> main

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_TIM_Base_Init ⇒ HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> TIM_Base_SetConfig
  - >> HAL_TIM_Base_MspInit
  [Called By]
  - >> main

  HAL_TIM_Base_MspInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> main

  HAL_TIM_ConfigClockSource (Thumb, 242 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> main

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 358 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  - >> HAL_TIMEx_CommutationCallback
  - >> HAL_TIMEx_BreakCallback
  [Called By]
  - >> TIM2_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HAL_UART_IRQHandler (Thumb, 218 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_Receive_IT
  [Calls]
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_ErrorCallback
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 94 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> UART_SetConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> main

  HAL_UART_MspInit (Thumb, 92 bytes, Stack size 32 bytes, stm32f1xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_RxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  LCD_DrawPixel (Thumb, 34 bytes, Stack size 8 bytes, spi_tft.o(i.LCD_DrawPixel))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_DrawPixel ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> LCD_SetCursorPosition
  - >> LCD_SendData
  - >> LCD_SendCommand
  [Called By]
  - >> line

  LCD_Fill (Thumb, 124 bytes, Stack size 24 bytes, spi_tft.o(i.LCD_Fill))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_Fill ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_SPI_Transmit_DMA
  - >> LCD_SetCursorPosition
  - >> LCD_SendCommand
  [Called By]
  - >> main

  LCD_Init (Thumb, 586 bytes, Stack size 8 bytes, spi_tft.o(i.LCD_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_Init ⇒ GPIO_init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_Delay
  - >> LCD_SendData
  - >> LCD_SendCommand
  - >> GPIO_init
  [Called By]
  - >> main

  LCD_SendCommand (Thumb, 46 bytes, Stack size 16 bytes, spi_tft.o(i.LCD_SendCommand))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SendCommand ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_SPI_Transmit_IT
  [Called By]
  - >> LCD_SetCursorPosition
  - >> LCD_DrawPixel
  - >> FONT_OUT
  - >> LCD_setOrientation
  - >> LCD_fillRect
  - >> LCD_Init
  - >> LCD_Fill

  LCD_SendData (Thumb, 46 bytes, Stack size 16 bytes, spi_tft.o(i.LCD_SendData))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_SPI_Transmit_IT
  [Called By]
  - >> LCD_SetCursorPosition
  - >> LCD_DrawPixel
  - >> LCD_setOrientation
  - >> LCD_Init

  LCD_SetCursorPosition (Thumb, 76 bytes, Stack size 24 bytes, spi_tft.o(i.LCD_SetCursorPosition))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> LCD_SendData
  - >> LCD_SendCommand
  [Called By]
  - >> LCD_DrawPixel
  - >> FONT_OUT
  - >> LCD_fillRect
  - >> LCD_Fill

  LCD_fillRect (Thumb, 192 bytes, Stack size 24 bytes, spi_tft.o(i.LCD_fillRect))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_SPI_Transmit_DMA
  - >> LCD_SetCursorPosition
  - >> LCD_SendCommand
  [Called By]
  - >> FONT_OUT
  - >> main

  LCD_setOrientation (Thumb, 46 bytes, Stack size 8 bytes, spi_tft.o(i.LCD_setOrientation))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_setOrientation ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> LCD_SendData
  - >> LCD_SendCommand
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = NMI_Handler ⇒ HAL_RCC_NMI_IRQHandler
  [Calls]
  - >> HAL_RCC_NMI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.RCC_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SPI1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI1_IRQHandler ⇒ HAL_SPI_IRQHandler
  [Calls]
  - >> HAL_SPI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  STRING_NUM_L (Thumb, 100 bytes, Stack size 48 bytes, spi_tft.o(i.STRING_NUM_L))
  [Stack]

  - Max Depth = 168
  - Call Chain = STRING_NUM_L ⇒ FONT_OUT ⇒ LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> FONT_OUT
  [Called By]
  - >> main

  STRING_OUT (Thumb, 56 bytes, Stack size 40 bytes, spi_tft.o(i.STRING_OUT))
  [Stack]

  - Max Depth = 160
  - Call Chain = STRING_OUT ⇒ FONT_OUT ⇒ LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> FONT_OUT
  [Called By]
  - >> main

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SystemClock_Config (Thumb, 126 bytes, Stack size 88 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 148
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_EnableCSS
  - >> HAL_RCC_ClockConfig
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_NVIC_SetPriority
  - >> HAL_RCCEx_PeriphCLKConfig
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  TIM2_IRQHandler (Thumb, 204 bytes, Stack size 40 bytes, stm32f1xx_it.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = TIM2_IRQHandler ⇒ HAL_TIM_IRQHandler
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  TIM_Base_SetConfig (Thumb, 86 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  USART1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_Receive_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  line (Thumb, 112 bytes, Stack size 40 bytes, spi_tft.o(i.line))
  [Stack]

  - Max Depth = 96
  - Call Chain = line ⇒ LCD_DrawPixel ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> LCD_DrawPixel
  [Called By]
  - >> main

  main (Thumb, 1354 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 192
  - Call Chain = main ⇒ STRING_NUM_L ⇒ FONT_OUT ⇒ LCD_fillRect ⇒ LCD_SetCursorPosition ⇒ LCD_SendData ⇒ HAL_SPI_Transmit_IT
  [Calls]
  - >> HAL_Delay
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_ReadPin
  - >> HAL_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_ADC_Stop
  - >> HAL_ADC_Start
  - >> HAL_ADC_PollForConversion
  - >> HAL_ADC_GetValue
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Start_IT
  - >> HAL_TIM_Base_Init
  - >> line
  - >> STRING_OUT
  - >> STRING_NUM_L
  - >> LCD_setOrientation
  - >> LCD_fillRect
  - >> LCD_Init
  - >> LCD_Fill
  - >> SystemClock_Config
  - >> FLASH_WriteSettings
  - >> FLASH_ReadSettings
  - >> MX_SPI1_Init
  - >> MX_GPIO_Init
  - >> MX_ADC1_Init
  - >> HAL_UART_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  FLASH_Program_HalfWord (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord))
  [Called By]

  - >> HAL_FLASH_Program_IT
  - >> HAL_FLASH_IRQHandler

  FLASH_SetErrorCode (Thumb, 60 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode))
  [Called By]

  - >> HAL_FLASH_IRQHandler

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  SPI_DMAError (Thumb, 30 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAError))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_DMAError
  [Calls]
  - >> HAL_SPI_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_DMAHalfTransmitCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_DMAHalfTransmitCplt
  [Calls]
  - >> HAL_SPI_TxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_DMATransmitCplt (Thumb, 108 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt))
  [Stack]

  - Max Depth = 48
  - Call Chain = SPI_DMATransmitCplt ⇒ SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_SPI_TxCpltCallback
  - >> HAL_SPI_ErrorCallback
  - >> SPI_WaitOnFlagUntilTimeout
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_TxCloseIRQHandler (Thumb, 130 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.SPI_TxCloseIRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = SPI_TxCloseIRQHandler ⇒ SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_SPI_TxRxCpltCallback
  - >> HAL_SPI_TxCpltCallback
  - >> HAL_SPI_ErrorCallback
  - >> SPI_WaitOnFlagUntilTimeout
  [Called By]
  - >> SPI_TxISR

  SPI_TxISR (Thumb, 66 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.SPI_TxISR))
  [Stack]

  - Max Depth = 48
  - Call Chain = SPI_TxISR ⇒ SPI_TxCloseIRQHandler ⇒ SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> SPI_TxCloseIRQHandler
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_IT)

  SPI_WaitOnFlagUntilTimeout (Thumb, 158 bytes, Stack size 32 bytes, stm32f1xx_hal_spi.o(i.SPI_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SPI_TxCloseIRQHandler
  - >> SPI_DMATransmitCplt

  DMA_SetConfig (Thumb, 30 bytes, Stack size 8 bytes, stm32f1xx_hal_dma.o(i.DMA_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_SetConfig
  [Called By]
  - >> HAL_DMA_Start_IT

  UART_Receive_IT (Thumb, 168 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 364 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 102 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  MX_ADC1_Init (Thumb, 58 bytes, Stack size 24 bytes, main.o(i.MX_ADC1_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_ADC1_Init ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_ADC_Init
  - >> HAL_ADC_ConfigChannel
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 178 bytes, Stack size 48 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_SPI1_Init (Thumb, 56 bytes, Stack size 8 bytes, main.o(i.MX_SPI1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_SPI1_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  [Called By]
  - >> main

  ### Undefined Global Symbols